[별표 3] 상태감시기록 및 분석 보고서(Trend Monitoring Recording and Analysis Report) 예시

OPERATOR: _________________________ TYPE OF OIL USED: ____________________________

Reg No.:    _________________________ S/N:  ____________________

MODEL NUMBER  ___________________ MFG.:  ___________________

DATE:  _________________________

TOTAL TIME: ___________________

TOH:  __________________________

INSPECTION INTERVAL (50 FH / 100 FH / ANUAL): _______________________

AREA #1

OIL ANALYSIS:	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
ALUMINUM
IRON
COPPER
SILICON
CHROMIUM
OIL PRESSURE
OIL TEMPERATURE
OIL FILTER
OIL SCREEN
OIL CONSUMPTION

AREA #2

	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
CHT
EGT#2

COMPRESSION

	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
#1
#2
#3
#4
#5
#6
#7
#8

DATE SPARK PLUG REPLACED _______________ @ ENGINE HOURS _____________

1 of 2

SPARK PLUG CONDITION:  1 = good,  2 = worn,  3 = oil fouled,  4 = carbon fouled

	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
#1 CYLINDER
TOP
BOTTOM
#2 CYLINDER
TOP
BOTTOM
#3 CYLINDER
TOP
BOTTOM
#4 CYLINDER
TOP
BOTTOM
#5 CYLINDER
TOP
BOTTOM
#6 CYLINDER
TOP
BOTTOM
#7 CYLINDER
TOP
BOTTOM
#8 CYLINDER
TOP
BOTTOM

	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
FUEL BURN
GPH

AREA #3 ACCESSORIES

	INSP. 1		INSP. 2		INSP. 3		INSP. 4		INSP. 5		INSP. 6		INSP. 7		INSP. 8
#1 CYLINDER	RT	LT	RT	LT	RT	LT	RT	LT	RT	LT	RT	LT	RT	LT	RT	LT
MAGNETO DROP@ 1500/1700 RPM
·······

	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
VACUUM GAUGE@ 1500/1700 RPM
ELECTRICAL VOLT/AMP @ 2100 RPM
·······

	INSP. 1	INSP. 2	INSP. 3	INSP. 4	INSP. 5	INSP. 6	INSP. 7	INSP. 8
AIR FILTER CONDITION
·······

DATE AIR FILTER REPLACED _____________________

2 of 2