【별표 3】서비스제공자의 안전성과지표를 구성하는 공통안전지표(Common Safety Indicator)

ㅇ 공통지표로 사용되는 위험사건(Hazard Event)

위험사건(72개)	위험도(발생빈도×심각도)			비율
	수용 (Acceptable)	유의 (Tolerable)
	낮은위험 (Minor)	중간위험 (Low Risk)	높은위험 (High Risk)
OE-05 - Fire/smoke/fumes warning	0.0%	0.0%	100.0%	0.28%
OE-04 - Engine fail/malfunction/fire	0.0%	0.0%	100.0%	0.11%
OE-09 - Over weight landing	0.0%	0.0%	100.0%	0.06%
OE-39 - Cabin pressure abnormal	0.0%	0.0%	100.0%	0.06%
OE-03 - Bird strike	0.0%	4.5%	95.5%	8.64%
OE-01 - In-flight engine shutdown	0.0%	33.3%	66.7%	0.17%
OE-31 - Execute emergency procedure	0.0%	33.3%	66.7%	0.17%
TE-19 - Part missing	0.0%	50.0%	50.0%	0.22%
OE-44 - A/C in-flight fire	0.0%	50.0%	50.0%	0.11%
TE-07 - Fuel system	5.9%	58.8%	35.3%	1.91%
TE-12 - Avionics	2.6%	64.1%	33.3%	2.19%
OE-17 - Fuel shortage	33.3%	33.3%	33.3%	0.17%
TE-04 - Equipment/furnishings	5.3%	63.2%	31.6%	1.07%
TE-05 - Fire protection	36.4%	36.4%	27.3%	1.23%
TE-01 - Air conditioning	13.3%	60.0%	26.7%	1.68%
GS-05 - Cargo /ULD shift by incorrect restraint	12.5%	62.5%	25.0%	0.45%
TE-16 - Doors / Window related event	19.4%	55.6%	25.0%	2.02%
TE-08 - Hydraulic system	18.8%	62.5%	18.8%	0.90%
GS-07 - Ground collision	33.3%	50.0%	16.7%	0.67%
TE-15 - Auxiliary Power Unit (APU)	66.7%	16.7%	16.7%	0.67%
OE-45 - A/C system warning	53.3%	33.3%	13.3%	0.84%
TE-10 - Gear & tire	19.5%	68.3%	12.2%	2.30%
TE-02 - Autopilot/FMS	75.0%	16.7%	8.3%	0.67%
OE-53 - Takeoff configuration warning	60.0%	33.3%	6.7%	0.84%
TE-17 - Engine related event	36.1%	57.4%	6.6%	3.42%
TE-03 - Electrical power	88.0%	8.0%	4.0%	1.40%
OE-60 - Weather encounter	73.2%	24.4%	2.4%	9.42%
TE-06 - Flight control	44.2%	53.5%	2.3%	2.41%
OE-42 - ACAS/TCAS triggered(RA)	31.3%	66.7%	2.1%	2.69%
TE-13 - Oxygen related event	0.0%	100.0%	0.0%	0.28%
OE-50 - Communication facility deficiency	0.0%	100.0%	0.0%	0.22%
OE-29 - Tire flat	0.0%	100.0%	0.0%	0.11%
GS-06 - Cargo related event by incorrect build-up	0.0%	100.0%	0.0%	0.06%
GS-13 - Weight and balance related event	0.0%	100.0%	0.0%	0.06%
OE-25 - Failure to comply SID	0.0%	100.0%	0.0%	0.06%
OE-51 - Abrupt maneuver	0.0%	100.0%	0.0%	0.06%
TE-14 - Pneumatic system fail	28.6%	71.4%	0.0%	0.79%
GS-14 - Ground Personnel Hazardous situation	33.3%	66.7%	0.0%	0.17%
GS-19 - Fuel Spill out	33.3%	66.7%	0.0%	0.17%
OE-37 - Exceeding the A/C operational limitations	40.0%	60.0%	0.0%	0.56%
TE-09 - Ice & rain protection	45.5%	54.5%	0.0%	0.62%
OE-47 - Aerodrome sys malfunction (NAV Aids)	50.0%	50.0%	0.0%	0.22%
CS-08 - In-flight Cabin crew illness/ incapacitation	50.0%	50.0%	0.0%	0.11%
OE-41 - Cockpit window crack	50.0%	50.0%	0.0%	0.11%
OE-55 - Ground collision during A/C operation	50.0%	50.0%	0.0%	0.11%
OE-61 - Documents & manuals	57.1%	42.9%	0.0%	0.39%
OE-43 - GPWS/EGPWS	65.4%	34.6%	0.0%	1.46%
TE-11 - Light related event	66.7%	33.3%	0.0%	0.34%
CS-01 - Cabin crew-hazardous situation	71.4%	28.6%	0.0%	0.39%
OE-52 - Deviation(by ATC instructions & procedures)	80.0%	20.0%	0.0%	0.28%
OE-63 - FOD(Foreign Object Damage)	90.0%	10.0%	0.0%	0.56%
OE-08 - Hard landing	94.4%	5.6%	0.0%	1.01%
CS-04 - In-flight Pax illness	98.7%	0.0%	1.3%	4.43%
CS-03 - In/voluntary pax deplane	97.6%	1.2%	1.2%	4.71%
CS-05 - Pax disturbance	97.2%	2.2%	0.6%	9.98%
CS-06 - Pax-hazardous Situation	97.4%	2.6%	0.0%	4.37%
CS-02 - Exit/entry door related	100.0%	0.0%	0.0%	0.45%
OE-48 - Airport operation facility	100.0%	0.0%	0.0%	0.45%
DG-02 - Incorrect loading	100.0%	0.0%	0.0%	0.11%
OE-32 - Airport close	100.0%	0.0%	0.0%	0.11%
OE-49 - Airspace _ ATS incident & communication error	100.0%	0.0%	0.0%	0.11%
TE-18 - Oil leak	100.0%	0.0%	0.0%	0.11%
DG-05 - Non-declaration	100.0%	0.0%	0.0%	0.06%
GS-01 - A/C engine suction	100.0%	0.0%	0.0%	0.06%
GS-02 - A/C floor parts damage	100.0%	0.0%	0.0%	0.06%
GS-04 - A/C wall damage	100.0%	0.0%	0.0%	0.06%
GS-08 - Ground near collision	100.0%	0.0%	0.0%	0.06%
OE-02 - Ground engine shutdown	100.0%	0.0%	0.0%	0.06%
OE-27 - Taxiway excursion	100.0%	0.0%	0.0%	0.06%
OE-46 - A/C navigation related event	100.0%	0.0%	0.0%	0.06%
OE-57 - Taxiway incursion	100.0%	0.0%	0.0%	0.06%
*SE-01 - Baggage reconciliation failure	33.3%	66.7%	0.0%	0.17%
*SE-02 - Watch list/no-fly/selectee irregularity	0.0%	0.0%	100.0%	0.06%
*SE-04 - Firearms handling irregularity	50.0%	50.0%	0.0%	0.11%
*SE-06 - Unauthorized person onboard	100.0%	0.0%	0.0%	0.17%
*SE-08 - No sealing on the catering carts or vehicles	100.0%	0.0%	0.0%	0.22%
*SE-09 - Air Taser related event	100.0%	0.0%	0.0%	0.34%
*SE-12 - Bomb threat	100.0%	0.0%	0.0%	0.06%
*SE-14 - Others	60.0%	40.0%	0.0%	0.28%
*OE-61 - Documents & manuals	57.1%	42.9%	0.0%	0.39%
*OE-62 - Miscellaneous	0.0%	100.0%	0.0%	0.11%
*OE-64 - Safety & Security Inspection	99.2%	0.8%	0.0%	6.84%
*OE-65 - Other operational event	9.1%	72.7%	18.2%	1.85%
*TE-20 - Other technical event	0.0%	85.7%	14.3%	1.18%
*GS-17 - Foreign CAB Inspection	15.5%	14.6%	69.9%	5.78%
*GS-18 - Other ground safety event	100.0%	0.0%	0.0%	0.50%
*CS-09 - Other cabin safety event	73.1%	23.1%	3.8%	1.46%

* 표시된 항목은 미적용

ㅇ 위해요인(Hazard) 분류코드

위해요인	위험사건(Hazard Event)	분류코드
OE-01-00	OE-01 - In-flight engine shutdown	-
OE-02-00	OE-02 - Ground engine shutdown	-
OE-03-00	OE-03 - Bird strike	-
OE-04-00	OE-04 - Engine fail/malfunction/fire	-
OE-05-00	OE-05 - Fire/smoke/fumes warning	-
OE-06-00	OE-06 - Stall warning(stick shaker)	-
OE-07-00	OE-07 - Wrong flap setting takeoff/landing	-
OE-08-00	OE-08 - Hard landing	-
OE-09-00	OE-09 - Over weight landing	-
OE-10-00	OE-10 - Gear-up landing	-
OE-11-00	OE-11 - Crab landing	-
OE-12-00	OE-12 - Forced landing(Intentional)	-
OE-13-00	OE-13 - Landing on beside landing surface	-
OE-14-00	OE-14 - Landing gear gravity extension	-
OE-15-00	OE-15 - Landing gear extended operation	-
OE-16-00	OE-16 - Takeoff on non-designated area	-
OE-17-00	OE-17 - Fuel shortage	-
OE-18-00	OE-18 - Incorrect fuel balance	-
OE-19-00	OE-19 - Overweight takeoff/incorrect CG(W&B)	-
OE-20-00	OE-20 - Overrun	-
OE-21-00	OE-21 - Undershoot	-
OE-22-00	OE-22 - Overshoot	-
OE-23-00	OE-23 - Tail skid/strike	-
OE-24-00	OE-24 - Near miss	-
OE-25-00	OE-25 - Failure to comply SID	-
OE-26-00	OE-26 - Runway excursion	-
OE-27-00	OE-27 - Taxiway excursion	-
OE-28-00	OE-28 - Apron excursion	-
OE-29-00	OE-29 - Tire flat	-
OE-30-00	OE-30 - Tire missing	-
OE-31-00	OE-31 - Execute emergency procedure	-
OE-32-00	OE-32 - Airport close	-
OE-33-00	OE-33 - Crash	-
OE-34-00	OE-34 - Computer Flight Plan/ATS Flight Plan	-
OE-35-00	OE-35 - Aircraft over-stress damage	-
OE-36-00	OE-36 - Exceeding approach & landing minima(CAT II, III & RVR)	-
OE-37-00	OE-37 - Exceeding the A/C operational limitations	-
OE-38-00	OE-38 - Explosive decompression damage	-
OE-39-00	OE-39 - Cabin pressure abnormal	-
OE-40-00	OE-40 - Flight crew incapacitation/illness	-
OE-41-00	OE-41 - Cockpit window crack	-
OE-42-00	OE-42 - ACAS/TCAS triggered(RA)	-
OE-43-01	OE-43 - GPWS/EGPWS	1. Glide slope
OE-43-02	OE-43 - GPWS/EGPWS	2. Sink rate
OE-43-03	OE-43 - GPWS/EGPWS	3. Landing gear
OE-43-04	OE-43 - GPWS/EGPWS	4. Flap
OE-43-05	OE-43 - GPWS/EGPWS	5. Terrain
OE-43-06	OE-43 - GPWS/EGPWS	6. Obstacle
OE-43-07	OE-43 - GPWS/EGPWS	7. Bank angle
OE-43-08	OE-43 - GPWS/EGPWS	8. Too low gear
OE-44-01	OE-44 - A/C in-flight fire	1. Cockpit
OE-44-02	OE-44 - A/C in-flight fire	2. Cabin
OE-44-03	OE-44 - A/C in-flight fire	3. Cargo compartment
OE-44-04	OE-44 - A/C in-flight fire	4. Others
OE-45-01	OE-45 - A/C system warning	1. Fuel system related warning
OE-45-02	OE-45 - A/C system warning	2. Landing gear system related warning
OE-45-03	OE-45 - A/C system warning	3. Air system related warning
OE-45-04	OE-45 - A/C system warning	4. Hydraulic system related warning
OE-45-05	OE-45 - A/C system warning	5. Avionics related warning
OE-45-06	OE-45 - A/C system warning	6. Flight control system related warning
OE-45-07	OE-45 - A/C system warning	7. Navigation system related warning
OE-45-08	OE-45 - A/C system warning	8. Cockpit / Cabin door System warning
OE-45-09	OE-45 - A/C system warning	9. Other system warning
OE-46-01	OE-46 - A/C navigation related event	1. Wrong aerodrome selected
OE-46-02	OE-46 - A/C navigation related event	2. Wrong runway selected
OE-46-03	OE-46 - A/C navigation related event	3. Wrong taxiway selected
OE-46-04	OE-46 - A/C navigation related event	4. Navigation track error
OE-46-05	OE-46 - A/C navigation related event	5. Others
OE-47-01	OE-47 - Aerodrome sys malfunction(NAV Aids)	1. Instrument landing sys
OE-47-02	OE-47 - Aerodrome sys malfunction(NAV Aids)	2. Global positioning sys
OE-47-03	OE-47 - Aerodrome sys malfunction(NAV Aids)	3. Marker beacon
OE-47-04	OE-47 - Aerodrome sys malfunction(NAV Aids)	4. Non-directional beacon
OE-47-05	OE-47 - Aerodrome sys malfunction(NAV Aids)	5. DME
OE-47-06	OE-47 - Aerodrome sys malfunction(NAV Aids)	6. VOR
OE-47-07	OE-47 - Aerodrome sys malfunction(NAV Aids)	7. PAPI/VASI
OE-47-08	OE-47 - Aerodrome sys malfunction(NAV Aids)	8. Precision approach radar
OE-48-01	OE-48 - Airport operation facility	1. VDGS
OE-48-02	OE-48 - Airport operation facility	2. Taxiway light
OE-48-03	OE-48 - Airport operation facility	3. Runway light
OE-48-04	OE-48 - Airport operation facility	4. Others
OE-49-01	OE-49 - Airspace _ ATS incident & communication error	1. Failure to comply STAR
OE-49-02	OE-49 - Airspace _ ATS incident & communication error	2. Failure to comply noise abatement procedure
OE-49-03	OE-49 - Airspace _ ATS incident & communication error	3. Airspace infringement (controlled/restricted/military)
OE-49-04	OE-49 - Airspace _ ATS incident & communication error	4. ATS Communications (crews, maint, controller, etc.)
OE-49-05	OE-49 - Airspace _ ATS incident & communication error	5. Incorrect clearance/instruction
OE-49-06	OE-49 - Airspace _ ATS incident & communication error	6. RVSM airspace incident
OE-49-07	OE-49 - Airspace _ ATS incident & communication error	7. Others
OE-50-01	OE-50 - Communication facility deficiency	1. HF communications
OE-50-02	OE-50 - Communication facility deficiency	2. VHF communications
OE-50-03	OE-50 - Communication facility deficiency	3. SATCOM
OE-50-04	OE-50 - Communication facility deficiency	4. Others
OE-51-01	OE-51 - Abrupt maneuver	1. Flight control
OE-51-02	OE-51 - Abrupt maneuver	2. Environment
OE-51-03	OE-51 - Abrupt maneuver	3. Crew
OE-51-04	OE-51 - Abrupt maneuver	4. Others
OE-52-01	OE-52 - Deviation(by ATC instructions & procedures)	1. Deviation-taxi
OE-52-02	OE-52 - Deviation(by ATC instructions & procedures)	2. Deviation-en-route
OE-52-03	OE-52 - Deviation(by ATC instructions & procedures)	3. Deviation-holding
OE-52-04	OE-52 - Deviation(by ATC instructions & procedures)	4. Deviation-runway crossing
OE-52-05	OE-52 - Deviation(by ATC instructions & procedures)	5. Deviation-clearance limit
OE-52-06	OE-52 - Deviation(by ATC instructions & procedures)	6. Deviation-flight level
OE-52-07	OE-52 - Deviation(by ATC instructions & procedures)	7. Deviation-assigned details
OE-52-08	OE-52 - Deviation(by ATC instructions & procedures)	8. Deviation-specified speed
OE-52-09	OE-52 - Deviation(by ATC instructions & procedures)	9. Deviation-time restriction
OE-53-01	OE-53 - Takeoff configuration warning	1. Flap
OE-53-02	OE-53 - Takeoff configuration warning	2. Speed brake
OE-53-03	OE-53 - Takeoff configuration warning	3. Stabilizer trim
OE-53-04	OE-53 - Takeoff configuration warning	4. Parking brake
OE-54-01	OE-54 - Collision during flight	1. to Aircraft (Mid-air collision)
OE-54-02	OE-54 - Collision during flight	2. to Vehicle
OE-54-03	OE-54 - Collision during flight	3. Equipment
OE-54-04	OE-54 - Collision during flight	4. Airport facility
OE-54-05	OE-54 - Collision during flight	5. Others
OE-55-01	OE-55 - Ground collision during A/C operation	1. to Aircraft
OE-55-02	OE-55 - Ground collision during A/C operation	2. to Vehicle
OE-55-03	OE-55 - Ground collision during A/C operation	3. to Equipment
OE-55-04	OE-55 - Ground collision during A/C operation	4. to Facility
OE-55-05	OE-55 - Ground collision during A/C operation	5. to Animal
OE-56-01	OE-56 - Near collision during A/C operation	1. to Aircraft
OE-56-02	OE-56 - Near collision during A/C operation	2. to Vehicle
OE-56-03	OE-56 - Near collision during A/C operation	3. to Equipment
OE-56-04	OE-56 - Near collision during A/C operation	4. to Facility
OE-56-05	OE-56 - Near collision during A/C operation	5. to Animal
OE-57-01	OE-57 - Taxiway incursion	1. By an aircraft
OE-57-02	OE-57 - Taxiway incursion	2. By a vehicle/equipment
OE-57-03	OE-57 - Taxiway incursion	3. By a person
OE-57-04	OE-57 - Taxiway incursion	4. By an animal
OE-58-01	OE-58 - Runway incursions	1. By an aircraft
OE-58-02	OE-58 - Runway incursions	2. By a vehicle/equipment
OE-58-03	OE-58 - Runway incursions	3. By a person
OE-58-04	OE-58 - Runway incursions	4. By an animal
OE-59-01	OE-59 - Apron incursion	1. By an aircraft
OE-59-02	OE-59 - Apron incursion	2. By a vehicle/equipment
OE-59-03	OE-59 - Apron incursion	3. By a person
OE-59-04	OE-59 - Apron incursion	4. By an animal
OE-60-01	OE-60 - Weather encounter	1. WX-Turbulence(include CAT)
OE-60-02	OE-60 - Weather encounter	2. WX-Lightning strike
OE-60-03	OE-60 - Weather encounter	3. WX-Thunderstorm
OE-60-04	OE-60 - Weather encounter	4. WX-Icing
OE-60-05	OE-60 - Weather encounter	5. WX-Vortex/Wake Turbulence
OE-60-06	OE-60 - Weather encounter	6. WX-Windshear
OE-60-07	OE-60 - Weather encounter	7. WX-Microburst
OE-60-08	OE-60 - Weather encounter	8. WX-Crosswind
OE-60-09	OE-60 - Weather encounter	9. WX-Tailwind
OE-60-10	OE-60 - Weather encounter	10. WX-Fog
OE-60-11	OE-60 - Weather encounter	11. WX-Hail
OE-60-12	OE-60 - Weather encounter	12. WX-Unexpected weather
OE-60-13	OE-60 - Weather encounter	13. Volcanic ash
OE-61-01	OE-61 - Documents & manuals	1. Required Documents
OE-61-02	OE-61 - Documents & manuals	2. Checklists
OE-61-03	OE-61 - Documents & manuals	3. Airway Manual (Jeppesen Chart)3. Airway Manual (Jeppesen Chart)
OE-61-04	OE-61 - Documents & manuals	4. Flight Operations Manual(FOM)
OE-61-05	OE-61 - Documents & manuals	5. AFM, FCOM, POM, QRH, ODM
OE-61-06	OE-61 - Documents & manuals	6. COM
OE-61-07	OE-61 - Documents & manuals	7. MEL
OE-61-08	OE-61 - Documents & manuals	8. NOTAM
OE-61-09	OE-61 - Documents & manuals	9. Load sheet
OE-61-10	OE-61 - Documents & manuals	10. DG/NOTOC
OE-61-11	OE-61 - Documents & manuals	11. Flight & Maintenance Log
OE-61-12	OE-61 - Documents & manuals	12. GD(General declaration)
OE-62-01	OE-62 - Miscellaneous	1. Crew coordination(Cockpit/Cabin)
OE-62-02	OE-62 - Miscellaneous	2. Crew rest seat
OE-62-03	OE-62 - Miscellaneous	3. Crew lay-over hotel
OE-62-04	OE-62 - Miscellaneous	4. Crew meal
OE-62-05	OE-62 - Miscellaneous	5. Crew schedule
OE-62-06	OE-62 - Miscellaneous	6. Crew Transition problem
OE-63-01	OE-63 - FOD(Foreign Object Damage)	1. Ice ball
OE-63-02	OE-63 - FOD(Foreign Object Damage)	2. Part from equipment
OE-63-03	OE-63 - FOD(Foreign Object Damage)	3. Part from aircraft
OE-63-04	OE-63 - FOD(Foreign Object Damage)	4. Stone
OE-63-05	OE-63 - FOD(Foreign Object Damage)	5. Other debris
OE-64-01	OE-64 - Safety & Security Inspection	-
OE-65-01	OE-65 - Other operational event	-
TE-01-01	TE-01 - Air conditioning	1. Cabin pressure all(Auto, manual) system
TE-01-02	TE-01 - Air conditioning	2. Cabin press auto control system
TE-01-03	TE-01 - Air conditioning	3. Air conditioning system
TE-01-04	TE-01 - Air conditioning	4. Air conditioning IND system
TE-01-05	TE-01 - Air conditioning	5. Others
TE-02-01	TE-02 - Autopilot/FMS	1. Auto pilot system both
TE-02-02	TE-02 - Autopilot/FMS	2. Autopilot/FMS components
TE-02-03	TE-02 - Autopilot/FMS	3. Autopilot/FMS IND system
TE-02-04	TE-02 - Autopilot/FMS	4. Others
TE-03-01	TE-03 - Electrical power	1. Emergency power
TE-03-02	TE-03 - Electrical power	2. Battery
TE-03-03	TE-03 - Electrical power	3. IDG/GEN
TE-03-04	TE-03 - Electrical power	4. External power
TE-03-05	TE-03 - Electrical power	5. Electrical power system
TE-03-06	TE-03 - Electrical power	6. Electrical power IND System
TE-03-07	TE-03 - Electrical power	7. Others
TE-04-01	TE-04 - Equipment/furnishings	1. Emergency equipment lose
TE-04-02	TE-04 - Equipment/furnishings	2. Emergency equipment damage
TE-04-03	TE-04 - Equipment/furnishings	3. Emergency equipment inop.
TE-04-04	TE-04 - Equipment/furnishings	4. Emergency equipment IND system
TE-04-05	TE-04 - Equipment/furnishings	5. Cockpit seat
TE-04-06	TE-04 - Equipment/furnishings	6. Lavatory system
TE-04-07	TE-04 - Equipment/furnishings	7. Galley system
TE-04-08	TE-04 - Equipment/furnishings	8. Escape slide unpack
TE-04-09	TE-04 - Equipment/furnishings	9. Others
TE-05-01	TE-05 - Fire protection	1. Fire bottle discharge
TE-05-02	TE-05 - Fire protection	2. Fire loop sys
TE-05-03	TE-05 - Fire protection	3. Fire IND sys
TE-05-04	TE-05 - Fire protection	4. Fire/smoke warning system components
TE-05-05	TE-05 - Fire protection	5. Fire/smoke warning system indication inop.
TE-05-06	TE-05 - Fire protection	6. Air/electric system fire/smoke false warning
TE-05-07	TE-05 - Fire protection	7. Others
TE-06-01	TE-06 - Flight control	1. Flap & slat asymmetry or jamming.
TE-06-02	TE-06 - Flight control	2. FLT control system actuator inop
TE-06-03	TE-06 - Flight control	3. FLT control system
TE-06-04	TE-06 - Flight control	4. FLT control IND system
TE-06-05	TE-06 - Flight control	5. Others
TE-07-01	TE-07 - Fuel system	1. Fuel leak
TE-07-02	TE-07 - Fuel system	2. Fuel spill out
TE-07-03	TE-07 - Fuel system	3. Fuel system unbalance
TE-07-04	TE-07 - Fuel system	4. Fueling sys
TE-07-05	TE-07 - Fuel system	5. Fuel contamination
TE-07-06	TE-07 - Fuel system	6. Fuel sys components
TE-07-07	TE-07 - Fuel system	7. Others
TE-08-01	TE-08 - Hydraulic system	1. HYD leak
TE-08-02	TE-08 - Hydraulic system	2. HYD tube chafing or damage
TE-08-03	TE-08 - Hydraulic system	3. HYD contamination
TE-08-04	TE-08 - Hydraulic system	4. HYD system
TE-08-05	TE-08 - Hydraulic system	5. HYD IND system
TE-08-06	TE-08 - Hydraulic system	6. Others
TE-09-01	TE-09 - Ice & rain protection	1. Pitot / static system
TE-09-02	TE-09 - Ice & rain protection	2. Pitot / static IND system
TE-09-03	TE-09 - Ice & rain protection	3. Engine cowl anti-ice system
TE-09-04	TE-09 - Ice & rain protection	4. Engine cowl anti-ice IND system
TE-09-05	TE-09 - Ice & rain protection	5. Windshield wiper system
TE-09-06	TE-09 - Ice & rain protection	6. Anti/De ice system components
TE-09-07	TE-09 - Ice & rain protection	7. Anti/De ice system indication
TE-09-08	TE-09 - Ice & rain protection	8. Others
TE-10-01	TE-10 - Gear & tire	1. Landing gear system
TE-10-02	TE-10 - Gear & tire	2. Landing gear IND system
TE-10-03	TE-10 - Gear & tire	3. Tire/brake system
TE-10-04	TE-10 - Gear & tire	4. Brake overheat
TE-10-05	TE-10 - Gear & tire	5. Auto brakes system inop
TE-10-06	TE-10 - Gear & tire	6. Tire fuse plugs melting
TE-10-07	TE-10 - Gear & tire	7. Anti-skid system
TE-10-08	TE-10 - Gear & tire	8. L/G steering system
TE-10-09	TE-10 - Gear & tire	9. Not remove - Ground lock pins
TE-10-10	TE-10 - Gear & tire	10. Others
TE-11-01	TE-11 - Light related event	1. Light system
TE-11-02	TE-11 - Light related event	2. Light IND system
TE-11-03	TE-11 - Light related event	3. Emergency exit light system
TE-11-04	TE-11 - Light related event	4. Cockpit light system
TE-11-05	TE-11 - Light related event	5. Cabin light system
TE-11-06	TE-11 - Light related event	6. Landing, Taxi, NAV light Inop.
TE-11-07	TE-11 - Light related event	7. A/C External Position Light Inop.
TE-11-08	TE-11 - Light related event	8. Others
TE-12-01	TE-12 - Avionics	1. Avionic system
TE-12-02	TE-12 - Avionics	2. Avionics IND system
TE-12-03	TE-12 - Avionics	3. Others
TE-13-01	TE-13 - Oxygen related event	1. Crew oxygen system
TE-13-02	TE-13 - Oxygen related event	2. PAX oxygen system
TE-13-03	TE-13 - Oxygen related event	3. Oxygen bottle press low
TE-13-04	TE-13 - Oxygen related event	4. Portable oxygen bottle press low
TE-13-05	TE-13 - Oxygen related event	5. Others
TE-14-01	TE-14 - Pneumatic system fail	1. Pneumatic system duct puncture/damage
TE-14-02	TE-14 - Pneumatic system fail	2. Pneumatic duct clamp damage
TE-14-03	TE-14 - Pneumatic system fail	3. Pneumatic system air leak
TE-14-04	TE-14 - Pneumatic system fail	4. Pneumatic system components
TE-14-05	TE-14 - Pneumatic system fail	5. Pneumatic system indication
TE-14-06	TE-14 - Pneumatic system fail	6. Others
TE-15-01	TE-15 - Auxiliary Power Unit (APU)	1. APU auto shut down
TE-15-02	TE-15 - Auxiliary Power Unit (APU)	2. APU bleed system
TE-15-03	TE-15 - Auxiliary Power Unit (APU)	3. APU generator system
TE-15-04	TE-15 - Auxiliary Power Unit (APU)	4. APU system components
TE-15-05	TE-15 - Auxiliary Power Unit (APU)	5. APU system indication
TE-15-06	TE-15 - Auxiliary Power Unit (APU)	6. Others
TE-16-01	TE-16 - Doors / Window related event	1. Pax door system
TE-16-02	TE-16 - Doors / Window related event	2. Pax door system IND
TE-16-03	TE-16 - Doors / Window related event	3. CGO door system
TE-16-04	TE-16 - Doors / Window related event	4. CGO door system IND
TE-16-05	TE-16 - Doors / Window related event	5. Cockpit Window
TE-16-06	TE-16 - Doors / Window related event	6. Others
TE-17-01	TE-17 - Engine related event	1. Engine surge
TE-17-02	TE-17 - Engine related event	2. Engine vibration system
TE-17-03	TE-17 - Engine related event	3. Engine fuel system components
TE-17-04	TE-17 - Engine related event	4. Engine oil system components
TE-17-05	TE-17 - Engine related event	5. Engine bleed air system components
TE-17-06	TE-17 - Engine related event	6. Engine control system components
TE-17-07	TE-17 - Engine related event	7. Engine starting system components
TE-17-08	TE-17 - Engine related event	8. Engine reverser system components
TE-17-09	TE-17 - Engine related event	9. Engine ignition system components
TE-17-10	TE-17 - Engine related event	10. Engine components
TE-17-11	TE-17 - Engine related event	11. Engine IND system components
TE-17-12	TE-17 - Engine related event	12. Others
TE-18-00	TE-18 - Oil leak	-
TE-19-00	TE-19 - Part missing	-
TE-20-00	TE-20 - Other technical event	-
CS-01-01	CS-01 - Cabin crew-hazardous situation	1. Contact with hot items(oven, beverage, etc.)
CS-01-02	CS-01 - Cabin crew-hazardous situation	2. Struck by objects(cart, baggage, etc.)
CS-01-03	CS-01 - Cabin crew-hazardous situation	3. Slip, trip, fall
CS-01-04	CS-01 - Cabin crew-hazardous situation	4. Non-standard surface(wet floor, step, etc.)
CS-01-05	CS-01 - Cabin crew-hazardous situation	5. Unstable Equipment handling
CS-01-06	CS-01 - Cabin crew-hazardous situation	6. Conduct with heavy-weight items
CS-01-07	CS-01 - Cabin crew-hazardous situation	7. Firm/hard landing
CS-01-08	CS-01 - Cabin crew-hazardous situation	8. Unexpected turbulence
CS-01-09	CS-01 - Cabin crew-hazardous situation	9. Other hazardous situation
CS-02-01	CS-02 - Exit/entry door related	1. Slide deployment (Mis-operation)
CS-02-02	CS-02 - Exit/entry door related	2. Improper door handling by pax
CS-02-03	CS-02 - Exit/entry door related	3. Inappropriate pax in exit row
CS-02-04	CS-02 - Exit/entry door related	4. Opened without cabin approval
CS-02-05	CS-02 - Exit/entry door related	5. Other door related event
CS-03-01	CS-03 - In/voluntary pax deplane	1. Refusal boarding
CS-03-02	CS-03 - In/voluntary pax deplane	2. Unexpected patient
CS-03-03	CS-03 - In/voluntary pax deplane	3. Personal reasons
CS-03-04	CS-03 - In/voluntary pax deplane	4. Other reasons
CS-04-01	CS-04 - In-flight Pax illness	1. Digestion disease
CS-04-02	CS-04 - In-flight Pax illness	2. Heart disease
CS-04-03	CS-04 - In-flight Pax illness	3. Fainting
CS-04-04	CS-04 - In-flight Pax illness	4. Respiratory disease
CS-04-05	CS-04 - In-flight Pax illness	5. Allergy(food poisoning)
CS-04-06	CS-04 - In-flight Pax illness	6. Other illness
CS-05-01	CS-05 - Pax disturbance	1. Smoking
CS-05-02	CS-05 - Pax disturbance	2. Verbal Abuse/Violent language
CS-05-03	CS-05 - Pax disturbance	3. Physical
CS-05-04	CS-05 - Pax disturbance	4. Drunken
CS-05-05	CS-05 - Pax disturbance	5. Sexual harassment
CS-05-06	CS-05 - Pax disturbance	6. Personal electronic devices
CS-05-07	CS-05 - Pax disturbance	7. Suspicious PAX
CS-05-08	CS-05 - Pax disturbance	8. Violent Yelling/Rage Expression
CS-05-09	CS-05 - Pax disturbance	9. Aircraft Illegal Occupation
CS-05-10	CS-05 - Pax disturbance	10. Violation of General Regulation
CS-05-11	CS-05 - Pax disturbance	11. Other pax disturbance
CS-06-01	CS-06 - Pax-hazardous Situation	1. Contact with hot items(beverage, etc.)
CS-06-02	CS-06 - Pax-hazardous Situation	2. Struck by objects(cart, falling baggage, etc.)
CS-06-03	CS-06 - Pax-hazardous Situation	3. Slip, trip, fall
CS-06-04	CS-06 - Pax-hazardous Situation	4. Non-standard surface(wet floor, step, etc.)
CS-06-05	CS-06 - Pax-hazardous Situation	5. Firm/hard landing
CS-06-06	CS-06 - Pax-hazardous Situation	6. Unexpected turbulence
CS-06-07	CS-06 - Pax-hazardous Situation	7. Other hazardous situation
CS-07-01	CS-07 - Safety duty related	1. Cabin crew/cabin not prepared for takeoff/landing
CS-07-02	CS-07 - Safety duty related	2. Pax not prepared for takeoff/landing
CS-07-03	CS-07 - Safety duty related	3. Other failure to perform safety duty
CS-08-00	CS-08 - In-flight Cabin crew illness/incapacitation	-
CS-09-00	CS-09 - Other cabin safety event	-
DG-01-01	DG-01 - Container/package breakage	1. Mishandling
DG-01-02	DG-01 - Container/package breakage	2. Incorrect B/UP
DG-02-01	DG-02 - Incorrect loading	1. CAO/MAG/Radioactive load to prohibited position
DG-02-02	DG-02 - Incorrect loading	2. Segregation violation
DG-02-03	DG-02 - Incorrect loading	3. Load unallowable DG to Pax flight
DG-03-01	DG-03 - Incorrect packaging	1. Shipper's mistake
DG-03-02	DG-03 - Incorrect packaging	2. Check error
DG-04-01	DG-04 - Miss-declaration	1. Shipper's mistake
DG-04-02	DG-04 - Miss-declaration	2. Check error
DG-05-01	DG-05 - Non-declaration	1. Shipper's mistake
DG-05-02	DG-05 - Non-declaration	2. Screening / MSDS check mistake
DG-06-01	DG-06 - Spill or leakage	1. Radiation
DG-06-02	DG-06 - Spill or leakage	2. Except radiation
DG-06-03	DG-06 - Spill or leakage	3. Mishandling
DG-06-04	DG-06 - Spill or leakage	4. Incorrect B/UP
DG-07-00	DG-07 - Other dangerous goods event	-
SE-01-00	SE-01 - Baggage reconciliation failure	-
SE-02-00	SE-02 - Watch list/no-fly/selectee irregularity	-
SE-03-00	SE-03 - Failure of baggage security inspection	-
SE-04-00	SE-04 - Firearms handling irregularity	-
SE-05-00	SE-05 - Failure of individual baggage check-in	-
SE-06-00	SE-06 - Unauthorized person onboard	-
SE-07-00	SE-07 - Improper security measures on passenger deplaning	-
SE-08-00	SE-08 - No sealing on the catering carts or vehicles	-
SE-09-01	SE-09 - Air Taser related event	1. No load due to ferry flight connection
SE-09-02	SE-09 - Air Taser related event	2. Malfunction of Air Taser box
SE-09-03	SE-09 - Air Taser related event	3. Other Air Taser handling irregularity
SE-10-00	SE-10 - Hijacking	-
SE-11-00	SE-11 - Unauthorized access to security controlled areas	-
SE-12-00	SE-12 - Bomb threat	-
SE-13-00	SE-13 - Suspicious items found	-
SE-14-00	SE-14 - Others	-
GS-01-01	GS-01 - A/C engine suction	1. Human
GS-01-02	GS-01 - A/C engine suction	2. Materials
GS-02-01	GS-02 - A/C floor parts damage	1. Incorrect shoring
GS-02-02	GS-02 - A/C floor parts damage	2. Incorrect weight balance inside ULD
GS-02-03	GS-02 - A/C floor parts damage	3. Use unserviceable ULD
GS-02-04	GS-02 - A/C floor parts damage	4. Violation of loading instruction
GS-02-05	GS-02 - A/C floor parts damage	5. Inexperience and mistake by G/H agent
GS-02-06	GS-02 - A/C floor parts damage	6. Leakage of salt water
GS-03-00	GS-03 - A/C tipping	1. Violation of loading/unloading Instruction
GS-04-01	GS-04 - A/C wall damage	1. Inexperience and mistake by G/H agent
GS-04-02	GS-04 - A/C wall damage	2. Skip Information from origin station
GS-04-03	GS-04 - A/C wall damage	3. B/UP height/length over than allowable contour
GS-04-04	GS-04 - A/C wall damage	4. Incorrect B/UP and restraint
GS-04-05	GS-04 - A/C wall damage	5. Shortage of 16ft & 20ft ULD
GS-05-01	GS-05 - Cargo /ULD shift by incorrect restraint	1. Improper locking
GS-05-02	GS-05 - Cargo /ULD shift by incorrect restraint	2. Mistake by G/H agent
GS-05-03	GS-05 - Cargo /ULD shift by incorrect restraint	3. Overlook at final check
GS-06-01	GS-06 - Cargo related event by incorrect build-up	1 .Mistake by W/H loader
GS-06-02	GS-06 - Cargo related event by incorrect build-up	2. Lack of training
GS-06-03	GS-06 - Cargo related event by incorrect build-up	3. Shortage of authorized tie-down equipment
GS-06-04	GS-06 - Cargo related event by incorrect build-up	4. Violation of B/UP instruction
GS-07-01	GS-07 - Ground collision	1. Aircraft to equipment/vehicle/facility
GS-07-02	GS-07 - Ground collision	2. Aircraft to aircraft while towing or pushback
GS-07-03	GS-07 - Ground collision	3. Vehicle to vehicle/equipment/facility
GS-07-04	GS-07 - Ground collision	4. Equipment to equipment/facility
GS-07-05	GS-07 - Ground collision	5. Others
GS-08-01	GS-08 - Ground near collision	1. Aircraft to equipment/vehicle/facility
GS-08-02	GS-08 - Ground near collision	2. Aircraft to aircraft while towing or pushback
GS-08-03	GS-08 - Ground near collision	3. Vehicle to vehicle/equipment/facility
GS-08-04	GS-08 - Ground near collision	4. Equipment to equipment/facility
GS-08-05	GS-08 - Ground near collision	5. Others
GS-09-01	GS-09 - Ground fire	1. Aircraft
GS-09-02	GS-09 - Ground fire	2. Equipment/vehicle
GS-09-03	GS-09 - Ground fire	3. Facilities
GS-10-01	GS-10 - Jet blast damage	1. Human
GS-10-02	GS-10 - Jet blast damage	2. Aircraft
GS-10-03	GS-10 - Jet blast damage	3. Vehicle
GS-10-04	GS-10 - Jet blast damage	4. Equipment
GS-10-05	GS-10 - Jet blast damage	5. Facility
GS-10-06	GS-10 - Jet blast damage	6. Others
GS-11-01	GS-11 - Pushback deficiency	1. Aircraft
GS-11-02	GS-11 - Pushback deficiency	2. Equipment
GS-11-03	GS-11 - Pushback deficiency	3. Human
GS-12-01	GS-12 - Towing deficiency	1. Aircraft
GS-12-02	GS-12 - Towing deficiency	2. Equipment
GS-12-03	GS-12 - Towing deficiency	3. Human
GS-13-01	GS-13 - Weight and balance related event	1. Weighing mistake
GS-13-02	GS-13 - Weight and balance related event	2. Weight misinformation from origin station
GS-13-03	GS-13 - Weight and balance related event	3. Mistype ULD number
GS-13-04	GS-13 - Weight and balance related event	4. Miscommunication between loader master and loader
GS-13-05	GS-13 - Weight and balance related event	5. Misread loading position
GS-13-06	GS-13 - Weight and balance related event	6 .Load wrong ULD due ground handling agent error
GS-13-07	GS-13 - Weight and balance related event	7. Skip final check of weight and balance
GS-13-08	GS-13 - Weight and balance related event	8. Overload
GS-13-09	GS-13 - Weight and balance related event	9. Over the a/c lateral imbalance weight
GS-13-10	GS-13 - Weight and balance related event	10. Over the a/c center of gravity zone
GS-13-11	GS-13 - Weight and balance related event	11. Over the a/c max structural limitations
GS-13-12	GS-13 - Weight and balance related event	12. Mis-input fuel data
GS-14-01	GS-14 - Ground Personnel Hazardous situation	1. hot items
GS-14-02	GS-14 - Ground Personnel Hazardous situation	2. Struck by objects (vehicle/equipment/facility etc)
GS-14-03	GS-14 - Ground Personnel Hazardous situation	3. Slip, trip, fall
GS-14-04	GS-14 - Ground Personnel Hazardous situation	4. Non-standard surface(wet floor, step, etc.)
GS-14-05	GS-14 - Ground Personnel Hazardous situation	5. Unstable Equipment handling
GS-14-06	GS-14 - Ground Personnel Hazardous situation	6. Conduct with heavy-weight items
GS-14-07	GS-14 - Ground Personnel Hazardous situation	7. Others
GS-15-01	GS-15 - Maintenance deficiency	1. Aircraft
GS-15-02	GS-15 - Maintenance deficiency	2. Engine
GS-15-03	GS-15 - Maintenance deficiency	3. Equipment
GS-15-04	GS-15 - Maintenance deficiency	4. Others
GS-16-01	GS-16 - Sabotage	-
GS-17-01	GS-17 - Foreign CAB Inspection	-
GS-18-01	GS-18 - Other ground safety event	-
GS-19-01	GS-19 - Fuel S+A23pill out	-

* OE : Operational Event

* TE : Technical Event

* CS : Cabin Safety Event

* DG : Dangerous Goods Event

* SE : Security Event

* GS : Ground Safety Event