항공구조구급대 운영 규정[별지 제16호서식]

탑재용 항공기 일지(제38조제1항 관련)

탑재용 항공기 일지

20   년도

○○○○항공구조구급대

257㎜×364㎜[백상지 80g/㎡]

○○○○소방항공대

항 공 기	등 록 부 호		등 록 년 월 일
	종 류		형 식
	감 항 유 별		형식증명서번호
	감항증명서번호		제 작 번 호
	항공기 제작자		제 작 년 월 일
발 동 기 형식 :	NO.1 일련번호		NO.2 일련번호
	NO.1 장착일자		NO.2 장착일자
	NO.1 장착시간		NO.2 장착시간
M / R 형식:	NO.1 일련번호		NO.2 일련번호
	NO.3 일련번호		NO.4 일련번호
	NO.5 일련번호		NO.6 일련번호
T / R 형식:
M G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
T G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
탑재용 항공일지 작성방법
비행일지기록사항	가. DUTY CODE IP : INSTRUCTOR P : CAPTAIN CP : CO-PILOT SP : STUDENT FE : FLIGHT ENGINEER R : RESCUE I : INSPECTOR PA : PASSENGER 나. 비행 중 결함은 정비일지 하단의 LEG NO. 란에 발생한 LEG의 숫자로 기록 후 서명하여야 한다. 다. DUTY CODE의 CAPTAIN은 매 비행 전 PILOT ACCEPTED란에 서명해야 한다. 라. ACTUAL TIME ; 항공기가 비행을 목적으로 이륙(바퀴가 땅에서 떨어지는 순간)하는 순간부터 착륙(바퀴가 땅에서 떨어지는 순간)할 때까지의 시간을 말한다. FLIGHT TIME ; 항공기가 엔진을 작동을 시작하는 시간부터 엔진이 멈출 때까지의 시간을 말함
정비일지기록사항	가. ENG OIL, G/B ; 그 날의 보급된 수량을 Q/T 또는 ℓ 로 기록한다. 나. DATE ; DAY - MON - YEAR ((예) 01 - JAN - 07)로 기록한다 ※ 시험비행(Test Flight or Function Check Flight); 실시한 작업의 결과에 대하여 감항성 및 비행성능을 확인하기 위하여 행하는 비행을 말한다. 주: 비행 중 시험(Flight Test)은 구조 및 성능 등에 대하여 비행 중 수행하는 시험을 말한다.

257㎜×364㎜[백상지 80g/㎡]

항 공 기	등 록 부 호		등 록 년 월 일
	종 류		형 식	AW139
	감 항 유 별		형식증명서번호
	감항증명서번호		일 련 번 호
	항공기 제작자		제 작 년 월 일
발 동 기 형식 : PT6C-67C	NO.1 일련번호		NO.2 일련번호
	NO.1 장착일자		NO.2 장착일자
	NO.1 장착시간		NO.2 장착시간
M / R 형식:3G6210A00131	NO.1 일련번호		NO.2 일련번호
	NO.3 일련번호		NO.4 일련번호
	NO.5 일련번호
T / R 형식:3G6410A00131	NO.1 일련번호		NO.2 일련번호
	NO.3 일련번호		NO.4 일련번호
M G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
I G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
T G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
탑재용 항공일지 작성방법
비행일지기록사항	가. DUTY CODE IP : INSTRUCTOR P : CAPTAIN CP : CO-PILOT SP : STUDENT FE : FLIGHT ENGINEER R : RESCUE I : INSPECTOR PA : PASSENGER 나. 비행 중 결함은 정비일지 하단의 LEG NO. 란에 발생한 LEG의 숫자로 기록 후 서명하여야 한다. 다. DUTY CODE의 CAPTAIN은 매 비행 전 PILOT ACCEPTED란에 서명해야 한다. 라. ACTUAL TIME ; 항공기가 비행을 목적으로 이륙(바퀴가 땅에서 떨어지는 순간)하는 순간부터 착륙(바퀴가 땅에서 떨어지는 순간)할 때까지의 시간을 말한다. FLIGHT TIME ; 항공기가 엔진을 작동을 시작하는 시간부터 엔진이 멈출 때까지의 시간을 말함
정비일지기록사항	가. ENG OIL, G/B ; 그 날의 보급된 수량을 Q/T 또는 ℓ 로 기록한다. 나. DATE ; DAY - MON - YEAR ((예) 01 - JAN - 07)로 기록한다 ※ 시험비행(Test Flight or Function Check Flight); 실시한 작업의 결과에 대하여 감항성 및 비행성능을 확인하기 위하여 행하는 비행을 말한다. 주: 비행 중 시험(Flight Test)은 구조 및 성능 등에 대하여 비행 중 수행하는 시험을 말한다.

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE	AS365N3	A/C NO.		DATE	- - DAY - MON- YEAR	/
ITEM	1	2	3	4	5
CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME
CREW NAME
LEG No.	PURPOSE OF FLT	STATION (FROM - TO)	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LANDING CYCLE	CAP'S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>	TOTAL		TOTAL
A/C TIME	No.1 ENGINE TIME	No.2 ENGINE TIME	LANDING CYCLE	EQUIPMENT CYCLE
HOIST	CARGO HOOK	SIMPLEX
TIME	START	GG Cycle	PT Cycle	TIME	START	GG Cycle	PT Cycle
PREV	:	:				:					/
TODAY	:	:				:					/
TOTAL	:	:				:					/
A/C RELEASE RECORDS	OIL(ℓ)	FUEL (ℓ)	SERVICED BY
LEG	MAINT DONE	DAY/ TIME	STA	MAINT RELEASE	A/C ACCEPTED BY	ENGINE(10ℓ)	MGB (10)	TGB (0.5)	HYD (8)	GRADE	SVC	TOTAL (1,158)	STA	BY
No.1 (5)	No.2 (5)
		/
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No.	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE		A/C NO.	HL9485	DATE	- - DAY - MON- YEAR	/
LEG No.	CREW NAME	PURPOSE OF FLT	STATION (FROM - TO)
1
2
3
4
5
LEG No.	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LAND CYCLE	CAT A TRAIN TIME	MTOW >6.4t TIME	WIND 27KNT NUM	CAP'S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>
A/C TIME	No.1 ENGINE TIME	No.2 ENGINE TIME	LAND CYCLE	EQUIPMENT CYCLE
HOIST	CARGO	BAMBI
START	TIME	START	TIME
PREV	:		:		:		/
TODAY	:		:		:		/
TOTAL	:		:		:		/
A/C RELEASE RECORDS	OIL(ℓ)	FUEL (ℓ)	SERVICED
LEG	MAINT DONE	DAY/ TIME	STA	MAINT RELEASE	A/C ACCEPTED	ENGINE(16ℓ)	MGB (19)	IGB (0.9)	TGB (1.5)	HYD(20)	GRADE	SVC	TOTAL (1,588)	STA	BY
No.1 (8)	No.2 (8)	PCM NO.1	PCM NO.2
		/
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No.	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE	BELL206L-3	A/C NO.		DATE	- - DAY - MON- YEAR	/
ITEM	1	2	3	4	5
CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME
CREW NAME
LEG No.	PURPOSE OF FLT	STATION (FROM - TO)	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LANDING CYCLE	CAP'S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>	TOTAL		TOTAL
ITEM	A/C TIME	ENGINE TIME	GRD TIME	LANDING CYCLE	RIN	EQUIPMENT CYCLE
CARGO HOOK	SIMPLEX
PREV	:	:	:
TODAY	:	:	:
TOTAL	:	:	:
LEG	MAINT DONE	DAY/TIME	STA	MAINT RELEASE	A/C ACCEPTED BY	OIL(Q/T)	FUEL (ℓ)	SERVICED BY
ENGINE (6)	X-MSN (5)	TGB (0.2)	HYD (0.5)	GRADE	SVC	TOTAL (416)	STA	BY
		/
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No.	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE	KA-32T	A/C NO.		DATE	- - DAY - MON- YEAR	/
ITEM	1	2	3	4	5
CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME
CREW NAME
LEG No.	PURPOSE OF FLT	STATION (FROM - TO)	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LANDING CYCLE	CAP'S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>	TOTAL		TOTAL
AIRFRAME TIME	PORT ENGINE TIME
ITEM	GRD RUN UP	FLT TIME	TOTAL TIME	LANDING CYCLE	GROUND RUN UP	FLIGHT TIME	After first OVHL	TOTAL TIME
TIME	T/O	NOMI'	TIME	T/O	NOMI'	CYCLE
PREV
TODAY
TOTAL
AI-9 ENGINE	MAIN ENGINE STARTING	STARBOARD ENGINE TIME
GROUND RUN UP	FLIGHT TIME	After first OVHL	TOTAL TIME
ITEM	STRATING	TIME	PORT	STBD	TIME	T/O	NOMI'	TIME	T/O	NOMI'	CYCLE
PREV
TODAY
TOTAL
GEAR BOX (BP-252)	EQUIP' CYCLE
ITEM	CYCLE	GROUND RUN UP	FLIGHT TIME	SINGLE ENG' IN FLIGHT	After first OVHL	TOTAL TIME	HOIST	CARGO HOOK	SIMPLEX
PORT	STBD
TIME	T/O	NOMI'	TIME	T/O	NOMI'	T/O	NOMI'	T/O	NOMI'
PREV
TODAY
TOTAL
LEG	MAINT DONE	DAY/ TIME	STA	MAINT RELEASE	A/C ACCEPTED BY	OIL(ℓ)	FUEL (ℓ)	SERVICED BY
PORT (16)	STBD (16)	AI-9 (2)	G/B (60)	HUB (19)	HYD (35)	BELLY (45)	GRADE	SVC	TOTAL (2,450)	STA	BY
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)