■ 119항공대 운영 규정 [별지 제12호서식] <종전의 서식 18호에서 이동>

탑재용 항공일지

20   년도

○○○○119항공대

257㎜×364㎜[백상지 80g/㎡]

○○○○119항공대

항 공 기	등 록 부 호		등 록 년 월 일
	종 류		형 식
	감 항 유 별		형식증명서번호
	감항증명서번호		제 작 번 호
	항공기 제작자		제 작 년 월 일
발 동 기 형식 :	NO.1 일련번호		NO.2 일련번호
	NO.1 장착일자		NO.2 장착일자
	NO.1 장착시간		NO.2 장착시간
M / R 형식:	NO.1 일련번호		NO.2 일련번호
	NO.3 일련번호		NO.4 일련번호
	NO.5 일련번호		NO.6 일련번호
T / R 형식:
M G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
T G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
탑재용 항공일지 작성방법
비행일지기록사항	가. DUTY CODE IP : INSTRUCTOR P : CAPTAIN CP : CO-PILOT SP : STUDENT FE : FLIGHT ENGINEER R : RESCUE I : INSPECTOR PA : PASSENGER 나. 비행 중 결함은 정비일지 하단의 LEG NO. 란에 발생한 LEG의 숫자로 기록 후 서명하여야 한다. 다. DUTY CODE의 CAPTAIN은 매 비행 전 PILOT ACCEPTED란에 서명해야 한다. 라. ACTUAL TIME ; 항공기가 비행을 목적으로 이륙(바퀴가 땅에서 떨어지는 순간)하는 순간부터 착륙(바퀴가 땅에서 떨어지는 순간)할 때까지의 시간을 말한다. FLIGHT TIME ; 항공기가 엔진을 작동을 시작하는 시간부터 엔진이 멈출 때까지의 시간을 말함
정비일지기록사항	가. ENG OIL, G/B ; 그 날의 보급된 수량을 Q/T 또는 ℓ 로 기록한다. 나. DATE ; DAY - MON - YEAR ((예) 01 - JAN - 07)로 기록한다 ※ 시험비행(Test Flight or Function Check Flight); 실시한 작업의 결과에 대하여 감항성 및 비행성능을 확인하기 위하여 행하는 비행을 말한다. 주: 비행 중 시험(Flight Test)은 구조 및 성능 등에 대하여 비행 중 수행하는 시험을 말한다.

257㎜×364㎜[백상지 80g/㎡]

항 공 기	등 록 부 호		등 록 년 월 일
	종 류		형 식	AW139
	감 항 유 별		형식증명서번호
	감항증명서번호		일 련 번 호
	항공기 제작자		제 작 년 월 일
발 동 기 형식 : PT6C-67C	NO.1 일련번호		NO.2 일련번호
	NO.1 장착일자		NO.2 장착일자
	NO.1 장착시간		NO.2 장착시간
M / R 형식:3G6210A00131	NO.1 일련번호		NO.2 일련번호
	NO.3 일련번호		NO.4 일련번호
	NO.5 일련번호
T / R 형식:3G6410A00131	NO.1 일련번호		NO.2 일련번호
	NO.3 일련번호		NO.4 일련번호
M G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
I G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
T G B	일 련 번 호		장 착 일 자
	장 착 시 간		형 식
탑재용 항공일지 작성방법
비행일지기록사항	가. DUTY CODE IP : INSTRUCTOR P : CAPTAIN CP : CO-PILOT SP : STUDENT FE : FLIGHT ENGINEER R : RESCUE I : INSPECTOR PA : PASSENGER 나. 비행 중 결함은 정비일지 하단의 LEG NO. 란에 발생한 LEG의 숫자로 기록 후 서명하여야 한다. 다. DUTY CODE의 CAPTAIN은 매 비행 전 PILOT ACCEPTED란에 서명해야 한다. 라. ACTUAL TIME ; 항공기가 비행을 목적으로 이륙(바퀴가 땅에서 떨어지는 순간)하는 순간부터 착륙(바퀴가 땅에서 떨어지는 순간)할 때까지의 시간을 말한다. FLIGHT TIME ; 항공기가 엔진을 작동을 시작하는 시간부터 엔진이 멈출 때까지의 시간을 말함
정비일지기록사항	가. ENG OIL, G/B ; 그 날의 보급된 수량을 Q/T 또는 ℓ 로 기록한다. 나. DATE ; DAY - MON - YEAR ((예) 01 - JAN - 07)로 기록한다 ※ 시험비행(Test Flight or Function Check Flight); 실시한 작업의 결과에 대하여 감항성 및 비행성능을 확인하기 위하여 행하는 비행을 말한다. 주: 비행 중 시험(Flight Test)은 구조 및 성능 등에 대하여 비행 중 수행하는 시험을 말한다.

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE	AS365N3	A/C NO.		DATE	- - DAY - MON- YEAR	/
ITEM	1	2	3	4	5
CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME
CREW NAME
LEG No.	PURPOSE OF FLT	STATION (FROM - TO)	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LANDING CYCLE	CAP’S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>	TOTAL		TOTAL
A/C TIME	No.1 ENGINE TIME	No.2 ENGINE TIME	LANDING CYCLE	EQUIPMENT CYCLE
HOIST	CARGO HOOK	SIMPLEX
TIME	START	GG Cycle	PT Cycle	TIME	START	GG Cycle	PT Cycle
PREV	:	:				:					/
TODAY	:	:				:					/
TOTAL	:	:				:					/
A/C RELEASE RECORDS	OIL(ℓ)	FUEL (ℓ)	SERVICED BY
LEG	MAINT DONE	DAY/ TIME	STA	MAINT RELEASE	A/C ACCEPTED BY	ENGINE(10ℓ)	MGB (10)	TGB (0.5)	HYD (8)	GRADE	SVC	TOTAL (1,158)	STA	BY
No.1 (5)	No.2 (5)
		/
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No.	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE		A/C NO.	HL9485	DATE	- - DAY - MON- YEAR	/
LEG No.	CREW NAME	PURPOSE OF FLT	STATION (FROM - TO)
1
2
3
4
5
LEG No.	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LAND CYCLE	CAT A TRAIN TIME	MTOW >6.4t TIME	WIND 27KNT NUM	CAP’S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>
A/C TIME	No.1 ENGINE TIME	No.2 ENGINE TIME	LAND CYCLE	EQUIPMENT CYCLE
HOIST	CARGO	BAMBI
START	TIME	START	TIME
PREV	:		:		:		/
TODAY	:		:		:		/
TOTAL	:		:		:		/
A/C RELEASE RECORDS	OIL(ℓ)	FUEL (ℓ)	SERVICED
LEG	MAINT DONE	DAY/ TIME	STA	MAINT RELEASE	A/C ACCEPTED	ENGINE(16ℓ)	MGB (19)	IGB (0.9)	TGB (1.5)	HYD(20)	GRADE	SVC	TOTAL (1,588)	STA	BY
No.1 (8)	No.2 (8)	PCM NO.1	PCM NO.2
		/
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No.	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE	BELL206L-3	A/C NO.		DATE	- - DAY - MON- YEAR	/
ITEM	1	2	3	4	5
CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME
CREW NAME
LEG No.	PURPOSE OF FLT	STATION (FROM - TO)	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LANDING CYCLE	CAP’S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>	TOTAL		TOTAL
ITEM	A/C TIME	ENGINE TIME	GRD TIME	LANDING CYCLE	RIN	EQUIPMENT CYCLE
CARGO HOOK	SIMPLEX
PREV	:	:	:
TODAY	:	:	:
TOTAL	:	:	:
LEG	MAINT DONE	DAY/TIME	STA	MAINT RELEASE	A/C ACCEPTED BY	OIL(Q/T)	FUEL (ℓ)	SERVICED BY
ENGINE (6)	X-MSN (5)	TGB (0.2)	HYD (0.5)	GRADE	SVC	TOTAL (416)	STA	BY
		/
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No.	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

257㎜×364㎜[백상지 80g/㎡]

FLT & MAINT LOG	A/C TYPE	KA-32T	A/C NO.		DATE	- - DAY - MON- YEAR	/
ITEM	1	2	3	4	5
CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME	CODE	NAME
CREW NAME
LEG No.	PURPOSE OF FLT	STATION (FROM - TO)	FLIGHT TIME	ACTUAL TIME	NIGHT TIME	INST TIME	LANDING CYCLE	CAP’S SIGN
R/O	R/I	F/T	T/O	L/D	A/T
1
2
3
4
5
<REMARKS>	TOTAL		TOTAL
AIRFRAME TIME	PORT ENGINE TIME
ITEM	GRD RUN UP	FLT TIME	TOTAL TIME	LANDING CYCLE	GROUND RUN UP	FLIGHT TIME	After first OVHL	TOTAL TIME
TIME	T/O	NOMI’	TIME	T/O	NOMI’	CYCLE
PREV
TODAY
TOTAL
AI-9 ENGINE	MAIN ENGINE STARTING	STARBOARD ENGINE TIME
GROUND RUN UP	FLIGHT TIME	After first OVHL	TOTAL TIME
ITEM	STRATING	TIME	PORT	STBD	TIME	T/O	NOMI’	TIME	T/O	NOMI’	CYCLE
PREV
TODAY
TOTAL
GEAR BOX (BP-252)	EQUIP’ CYCLE
ITEM	CYCLE	GROUND RUN UP	FLIGHT TIME	SINGLE ENG’ IN FLIGHT	After first OVHL	TOTAL TIME	HOIST	CARGO HOOK	SIMPLEX
PORT	STBD
TIME	T/O	NOMI’	TIME	T/O	NOMI’	T/O	NOMI’	T/O	NOMI’
PREV
TODAY
TOTAL
LEG	MAINT DONE	DAY/ TIME	STA	MAINT RELEASE	A/C ACCEPTED BY	OIL(ℓ)	FUEL (ℓ)	SERVICED BY
PORT (16)	STBD (16)	AI-9 (2)	G/B (60)	HUB (19)	HYD (35)	BELLY (45)	GRADE	SVC	TOTAL (2,450)	STA	BY
		/
		/
		/
		/
TOTAL
SCHEDULE CHECK DUE	PART CHANGE RECORDS
TYPE	DUE TIME	DUE DATE	COMPLETE	ITEM	KEY WORD	PART NO	POS	S/N ON	S/N OFF
LEG No.	ITEM No	ORDER DESCRIPTION	CORRECTIVE ACTION(STA, DATE, SIGNATURE, CERT No, etc)

FLT & MAINT LOG	A/C TYPE AW169	REG No / CALL SIGN	YEAR MONTH DAY 20 . .	0	1
2	3
A/C RELLEASE	CPTN SIGN	CREW NAME	DUTY CODE	REMARK
LEG	INSP	MTH	DATE	STA	TECHNICIAN	PILOT	LEG
BY	LIC	BY	LIC	1	2	3	4	5	6
LEG	FLIGHT STATUS	L/D CYL	Cat.A FH	4,600 FH	4,600 L/D	CREW	FLT PURPOSE
FR	TO	R/O	R/I	B/T	T/O	L/D	F/T	NGT	INST
T/O	L/D
TTL
SEC	AIRFRAME	ENGINE No.1	ENGINE NO.2	HOIST	CARGO HOOK(BUCKET)
L/D	FH	CYL	FH	CYL	FH	LIFT	OPT	LIFT	FH
PRE
TDY
TTL
LEG	FUEL(ℓ) JET A-1	LUBRICANT & HYD FLUID(ℓ)	SERVICED
EASTMAN TO 2380	SHEEL 555	SHELL 31	SEC	STA	BY
SVC	TTL	ENG No.1	ENG No.2	MGB	IGB	TGB	HYD SYS
SVC	IN	SVC	IN	SVC	IN	SVC	IN	SVC	IN	SVC	IN
PRE
PARTS CHANGE RECORD
PARE NAME	P/N	OFF (S/N)	ON (S/N)	POSITION	KEY WORD
LEG	ITEM	MALFUNCTION (DATE, STA, DUTY, NAME, LIC, NO etc...)	LEG	ITEM	CORRECTIVE ACTION (DATE, STA, DUTY, NAME, LIC, NO etc...)

FLT & MAINT LOG	A/C TYPE KA-32T	REG No / CALL SIGN	YEAR MONTH DAY 20 . .	0	1
2	3
A/C RELEASE	CPTN SIGN	CREW NAME	DUTY CODE	REMARK
LEG	INSP	MTH	DATE	STA	TECHNICIAN	PILOT	LEG
1	2	3	4
BY	LIC	BY	LIC
LEG	FLIGHT STATUS	CREW	FLIGHT PURPOSE
FR	TO	R/O	R/I	B/T	T/O	L/D	F/T	NGT	INST	L/D	CRG	T/O	L/D
TTL
SEC	AIRFRAME	ENGINE (PORT) : ТВ3-117ВМА ser 02
L/D	GRD	FLT	TTL	CYL	GRD	FLT	TTL
HEL	RUN	FLT	CRG	TIME	NML	T/O	TIME	NML	T/O
PRE
TDY
TTL
SEC	A.P.U : АИ-9	ENGINE (STBD) : ТВ3-117ВМА ser 02
START	OPT	MAIN ENG START	CYL	GRD	FLT	TTL
PORT	STBD	FLT	CRG	TIME	NML	T/O	TIME	NML	T/O
PRE
TDY
TTL
SEC	GEAR BOX : ВР-252	HOIST CYL
GRD	FLT	SEIF (PORT)	SEIF (STBD)	TTL
TIME	NML	T/O	TIME	NML	T/O	CRU	NML	T/O	CRU	NML	T/O
PRE
TDY
TTL
LEG	FUEL (ℓ) JET A-1(JP-8)	OIL (ℓ)	HYD (ℓ)	SERVICED
JET OIL 254	BO-12	ROYCO 756	SEC	STA	BY
SVC	TTL	ENG PORT	ENG STBD	A.P.U	G.B	HUB	A/C
PRE
PARTS CHANGE RECORD
PART NAME	P/N	OFF (S/N)	ON (S/N)	POSITION	KEY WORD
LEG	ITEM	MALFUNCTION (DATE, STA, DUTY, NAME, LIC No etc...)	LEG	ITEM	CORRECTIVE ACTION (DATE, STA, DUTY, NAME, LIC No etc...)

※ 기종에 따라 서식 작성이 어려운 경우 일부 내용 수정 작성 가능